

PHONE: 304-325-7323 FAX: 304-325-6525

WEBSITE: [WWW.RITCHIEEQUIPMENT.COM](http://WWW.RITCHIEEQUIPMENT.COM)

EMAIL: [PATRIOTEQUIPSALES@OUTLOOK.COM](mailto:PATRIOTEQUIPSALES@OUTLOOK.COM)

PATRIOT SALES & SERVICE, LLC

1244 MERCER MALL ROAD BLUEFILED, WV 24701

**1999 INT. 2674 6X6 TANDEM AXLE DERRICK TK. $57,500.00**

**S/N 1HTGLAHT5XH679661**

**W/ ALTEC MODEL #4060ATR BODY**

**MILES: 73,912**

**HOURS: 3827**

**6X6**

**CUMMINS ISM 350 ENGINE 350 H.P.**

**10 SPEED SPICER MANUAL TRANSMISSION MODEL #PSO150-10SP1 S/N ASMG104880-1**

**FRONT TRANSFER CASE REBUILT PER PREVIOUS OWNER**

**214” WHEEL BASE**

**TIRES: RF BRIDGESTONE 315/80R225 M870 APPROX. 90%**

**LF BRIDGESTONE 315/80R225 M870 APPROX. 90%**

**RRFO BRIDGESTONE 11R 22.5 M770 APPROX. 65%**

**RRFI MICHELIN 11R 22.5 XDE APPROX. 65%**

**RRRO CONTINENTAL 11R 22.5 HDR2 APPROX. 65%**

**RRRI YOKOHAMA 11R 22.5 RY 617 APPROX. 65%**

**LRFO FIRESTONE 11R 22.5 FD 663 APPROX. 65%**

**LRFI GOODYEAR 11R 22.5 G622 APPROX. 50%**

**LRRO GOODYEAR 11R 22.5 G182 RSD APPROX. 40%**

**LRRI FIRESTONE 11R 22.5 FD 663 APPROX. 65%**

**WIRELESS REMOTE**

**SPARE REMOTE BATTERY AND CHARGER**

**FRONT BUMPER PULL RING**

**ALTEC BED S/N 17-57888 11/99**

* **REMOVEABLE SIDE BOARDS**
* **TOOLBOXES**
* **UNDER DECK STORAGE 12”H X 24”W X 89”L**
* **CHOCK AND OUTRIGGER PAD STORAGE**
* **DECK STORAGE BRACKETS**
* **ADJUSTABLE POLE RACK W/ RACHET STRAPS**

**ALTEC MODEL #4060ATR S/N #0411DF0403**

* **MAX REACH 60’**
* **MAXIMUM LIFT CAPACITY: 30,000 LBS.**
* **MAXIMUM HORRIZONTAL REACH FROM CENTERLINE OF ROTATION 50.3’**

**PAGE 1 OF 2**

* **BOOM ARTICULATION 15 TO 80 DEGREES**
* **DIGGING RADIUS MIN. 22’**
* **DIGGING RADIUS MAX. 35.2’**
* **MULTI LEVER CONTROL STATION RIDING SEAT**
* **FIVE FUNCTION HYD. OVERLOAD PROTECTION SYSTEM**
* **STANDARD / LOW SPEED SELECTOR**
* **INSULATING FIBERGLASS THIRD STAGE, RATED TO 46KV AND BELOW**
* **FIBERGLASS BOOM TIP AND TRANSFERABLE STEEL BOOM FLARES**
* **HYDRAULIC SIDE LOAD PROTECTION**
* **15,000# WORM GEAR TURNTABLE WINCH WITH ROPE GUIDES**
* **HYDRAULIC TILTING POLE GUIDES WITH INTERLOCK**
* **12,OOO FT-LBS DIGGER MOTOR, TWO SPEED MECHANICAL SHIFT**
* **HYDRAULIC AUGER RELEASE**
* **BOOM AND AUGER STOW PROTECTION**
* **TOOL CIRCUIT**
* **MATERIAL HANDLING JIB**
* **FRONT AND REAR OUTRIGGERS**
* **300# CAPACITY WORK BUCKET**
* **SPARE MATERIAL HANDLING JIB**
* **SPARE POLE RACK ARMS**

**AIR AND POWER FOR AUXILILARY TRAILER**

**PINTLE HOOK**

**HYD. TOOL CIRCUIT**

**STROBE HAZARD LIGHTS**

**FIRE EXT.**

**WORK LIGHTS**

**SERVICED**

**WORK READY**

**GOOD CONDITION**

**FOR MORE INFORMATION AND TO VIEW EQUIPMENT, PLEASE VISIT** [**WWW.RITCHIEEQUIPMENT.COM**](http://WWW.RITCHIEEQUIPMENT.COM) **\*PRICES AND SPECIFICATIONS ARE SUBJECT TO CHANGE WITHOUT NOTICE\***